Kofiko-Intan tips:

1. Ground everything possible to the wiz box (screen, cables, wall ground).
2. Connect both Ground & Reference to the reference electrode in saline
3. Make sure the cable of the electrode doesn’t form a circle or a very long antennae
4. Connect the USB shield to the local aluminium foil.